TINTED HARD WAX OIL

A blend of natural oils and waxes offering exceptional durability and resistance for internal timber surfaces including floors, bench tops, furniture and areas subjected to a high degree of wear.

Produces a quick drying natural matt, silk, satin or gloss water repellent, tread-fast finish that will not peel or flake. Hard Wax Oil is easy to maintain and as a natural replenishable product it is easy to rejuvenate timber when required.

**Preparation**

Ensure all surfaces are clean, dry and free from previous finish. Minor gaps and holes can be filled with Fiddes Filler Gel if required. Sand the substrate with a fine 120-150 grade sandpaper. Ensure the surface is clean and remove all traces of dust prior to application.

**Application**

Ensure all areas to be coated are extremely well ventilated during and after application and always test on a small area prior to use. No sealer or primer is required. Stir contents thoroughly before and during use. Maximum 2 coats recommended. Clean applicators with White Spirits.

***Floors*** -

Apply with a brush, trowel or a floor applicator and buff in with a TAN or BEIGE floor pad using a slow speed buffing machine (175 RPM) whilst ragging edges working the product across the floor. Once dry, apply a coat of clear Hard Wax Oil using a short nap microfibre roller. Alternatively, to achieve a similar look without using a buffing machine mix 10% Tinted HWO with clear HWO and roll on using a short nap microfibre roller.

You can also roll the Tinted HWO straight using a short nap microfibre roller being extremely careful not to overlap and to leave roller stop marks.

***Furniture*** -

Brush or roll the Tinted Hard Wax Oil and then using a rag, buff into the surface ensuring the entire surface has been covered. Once dry, apply a coat of clear Hard Wax Oil using a short nap microfibre roller. Alternatively, see above instructions to mix Tinted with Clear Hard Wax Oil.

**Additional notes**

\*When applied using the above methods the Tinted Hard Wax Oil is more of a transparent tint. If the project requires a deeper colour we recommend using a direct stain such as Fiddes Nitro or Light Fast Water Stain before applying a Clear Hard Wax Oil as per instructions.

\*Always do a test patch first and ensure the substrate is prepared in the same process as the project will be completed.

\*Please refer to the Hard Wax Oil Application Sheet for additional application information.